/*
    FreeRTOS V6.0.2 - Copyright (C) 2010 Real Time Engineers Ltd.

    ***************************************************************************
    *                                                                         *
    * If you are:                                                             *
    *                                                                         *
    *    + New to FreeRTOS,                                                   *
    *    + Wanting to learn FreeRTOS or multitasking in general quickly       *
    *    + Looking for basic training,                                        *
    *    + Wanting to improve your FreeRTOS skills and productivity           *
    *                                                                         *
    * then take a look at the FreeRTOS eBook                                  *
    *                                                                         *
    *        "Using the FreeRTOS Real Time Kernel - a Practical Guide"        *
    *                  http://www.FreeRTOS.org/Documentation                  *
    *                                                                         *
    * A pdf reference manual is also available.  Both are usually delivered   *
    * to your inbox within 20 minutes to two hours when purchased between 8am *
    * and 8pm GMT (although please allow up to 24 hours in case of            *
    * exceptional circumstances).  Thank you for your support!                *
    *                                                                         *
    ***************************************************************************

    This file is part of the FreeRTOS distribution.

    FreeRTOS is free software; you can redistribute it and/or modify it under
    the terms of the GNU General Public License (version 2) as published by the
    Free Software Foundation AND MODIFIED BY the FreeRTOS exception.
    ***NOTE*** The exception to the GPL is included to allow you to distribute
    a combined work that includes FreeRTOS without being obliged to provide the
    source code for proprietary components outside of the FreeRTOS kernel.
    FreeRTOS is distributed in the hope that it will be useful, but WITHOUT
    ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or
    FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License for
    more details. You should have received a copy of the GNU General Public 
    License and the FreeRTOS license exception along with FreeRTOS; if not it 
    can be viewed here: http://www.freertos.org/a00114.html and also obtained 
    by writing to Richard Barry, contact details for whom are available on the
    FreeRTOS WEB site.

    1 tab == 4 spaces!

    http://www.FreeRTOS.org - Documentation, latest information, license and
    contact details.

    http://www.SafeRTOS.com - A version that is certified for use in safety
    critical systems.

    http://www.OpenRTOS.com - Commercial support, development, porting,
    licensing and training services.
*/
#include "FreeRTOSConfig.h"
#include "portasm.h"

	IMPORT vTaskIncrementTick
	IMPORT vTaskSwitchContext
	IMPORT vPortSetupTimerInterrupt

	EXPORT vTickISR
	EXPORT vPortYield
	EXPORT xPortStartScheduler
	
	RSEG CODE

/*
 * The RTOS tick ISR.
 *
 * If the cooperative scheduler is in use this simply increments the tick
 * count.
 *
 * If the preemptive scheduler is in use a context switch can also occur.
 */
vTickISR:
	portSAVE_CONTEXT
				
	call	#vTaskIncrementTick

	#if configUSE_PREEMPTION == 1
		call	#vTaskSwitchContext
	#endif
		
	portRESTORE_CONTEXT
/*-----------------------------------------------------------*/


/*
 * Manual context switch called by the portYIELD() macro.
 */
vPortYield:

	/* Mimic an interrupt by pushing the SR. */
	push	SR			

	/* Now the SR is stacked we can disable interrupts. */
	dint			
				
	/* Save the context of the current task. */
	portSAVE_CONTEXT			

	/* Switch to the highest priority task that is ready to run. */
	call	#vTaskSwitchContext		

	/* Restore the context of the new task. */
	portRESTORE_CONTEXT
/*-----------------------------------------------------------*/


/*
 * Start off the scheduler by initialising the RTOS tick timer, then restoring
 * the context of the first task.
 */
xPortStartScheduler:

	/* Setup the hardware to generate the tick.  Interrupts are disabled
	when this function is called. */
	call	#vPortSetupTimerInterrupt

	/* Restore the context of the first task that is going to run. */
	portRESTORE_CONTEXT
/*-----------------------------------------------------------*/
      		

	/* Install vTickISR as the timer A0 interrupt. */
	ASEG
	ORG 0xFFE0 + TIMERA0_VECTOR
	
	_vTickISR_: DC16 vTickISR
	

	END
		
